Approved by the order of the Chairman of "Azerbaijan Caspian Shipping Closed Joint Stock Company dated 1st of December 2016No. 216.



**AZERBAIJAN CASPIAN SHIPPING CLOSED JOINT STOCK COMPANY IS ANNOUNCING OPEN BIDDING FOR THE PROCUREMENT OF HOSES OF VARIOUS PURPOSE REQUIRED FOR STRUCTURAL DEPARTMENTS OF ASCO**

**B I D D I N G No. AM069 / 2023**

|  |  |
| --- | --- |
|  | **Submission documentation required for participation in the bidding:**   * Application for participation in the bidding (template has been attached hereto); * Bank evidence as a proof of participation fee; * Bidding offer: * Bank document confirming financial condition of the consignor within the last year (or within the period of operation if less than one year); * Statement issued by the relevant tax authorities on the absence of expired commitments associated with taxes and other compulsory payments and failure of obligations set forth in the Tax Code of the Republic of Azerbaijan for the last one year (excluding the period of suspension).   At the initial stage, application for participation in the bidding ( signed and stamped ) and bank evidence proving payment of participation fee (excluding bidding offer) shall be submitted in English, Russian or in Azerbaijani languages to the official address of "Azerbaijan Caspian Shipping" CJSC (hereinafter referred to as "ASCO" or "Procuring Organization") through email address of contact person in charge by 17.00 (Baku time) **on 28th of April 2023**. Whereas, other necessary documents shall be submitted as enclosed in the bidding offer envelope.    Description (list) of goods, works or services has been attached hereto. |
|  | **The participation fee and Collection of General Terms and Conditions:**   * Any participant (bidder), who desires to participate in the bidding, shall pay for participation fee stated below *(the payment order shall necessarily state the name of the organization holding open bidding and the subject of the bidding)* and shall submit the evidence as a proof of payment to ASCO not later than the date stipulated in section one. All participants (bidders), who have fulfilled these requirements, may obtain General Terms and Conditions relating to the procurement subject from the contact person in charge by the date envisaged in section IV of this announcement at any time from 09.00 till 18.00 in any business day of a week. * Participation fee amount (VAT exclusive): AZN 50 * The participation fee may be paid in AZN or equivalent amount thereof in USD or EURO. * ***Account No. :***  |  |  |  | | --- | --- | --- | | AZN | USD | EURO | | Name: The International Bank of Azerbaijan  ABB- Customer Service Department  Code: 805250  TAX ID: 9900001881  Correspondent account: AZ03NABZ01350100000000002944  SWIFT: IBAZAZ2X  Beneficiary: AZARB.XAZAR DANIZ GAMICILIYI QSC  TAX ID: 1701579951  Account No. (AZN): AZ36IBAZ38050019441115341120 | Intermediary Bank: Citibank N.Y,  New York  Acc.36083186, SWIFT: CITIUS33  Beneficiary Bank: The International Bank of Azerbaijan  IBA- Customer Service Department  SWIFT: IBAZAZ2X  Nizami str., 67 Beneficiary: AZARB.XAZAR DANIZ GAMICILIYI QSC  TAX ID: 1701579951  Account No.: AZ26IBAZ38150018401115341120 | Intermediary Bank: Commerzbank AG, Frankfurt am Main  SWIFT: COBADEFF  ACC # 400 88 660 3001  Beneficiary Bank: The International Bank of Azerbaijan,  IBA-Premier Customer Service SWIFT: IBAZAZ2X Nizami str., 67 Beneficiary: Azerbaijan Caspian Shipping CJSC  TAX ID: 1701579951  Account No.: AZ06IBAZ38150019781115341120 |  * **Except for circumstances where the bidding is cancelled by ASCO, participation fee shall in no case be refunded!** |
|  | **Security for a bidding offer:**   * The bank guarantee is required in the amount of at least 1 (one) % of the bidding offer price. A bank guarantee sample shall be specified in the General Terms and Conditions. * Bank guarantees shall be submitted as enclosed in the bidding offer envelope along with the bidding offer. Otherwise, the Purchasing Organization shall reserve the right to reject such offer. * The financial institution that issued the guarantee should be acknowledged in the Republic of Azerbaijan and / or international financial transactions. The purchasing organization shall reserve the right not to accept and reject any unreliable bank guarantee. * Persons wishing to participate in the bidding and intending to submit another type of warranty (letter of credit, securities, transfer of funds to the special banking account set forth by the Procuring Organization in the bidding documents, deposit and other financial assets) shall request and obtain a consent from ASCO through the contact person reflected in the announcement on the acceptability of such type of warranty. * A contract performance bond is required in the amount of 5 (five) % of the purchase price. * For the current procurement operation, the Procuring Organization is expected to make payment only after the goods have been delivered to the warehouse, no advance payment has been intended. |
|  | **Final deadline date and time for submission of the bidding offer:**   * All participants, which have submitted their application for participation in the bidding and bank evidence as a proof of payment of participation fee by the date and time stipulated in section one, and shall submit their bidding offer (one original and two copies) enclosed in sealed envelope to ASCO by **17.00** Baku time on **May 3, 2023.** * All bidding offer envelopes submitted after the above-mentioned date and time shall be returned unopened. |
|  | **Address of the procuring company:**  The Azerbaijan Republic, Baku city, AZ1029 (postcode), 2 Neftchilar Avenue, Procurement Committee of ASCO.  **Contact person in charge:**  Rahim Abbasov  Procurement specialist at the Procurement Department of ASCO  Telephone No.: **+99450 2740277**  Email address: rahim.abbasov@asco.az, [tender@asco.az](mailto:tender@asco.az)  **Contact person on legal issues:**  Landline No.: +994 12 4043700 (ext: 1262)  Email address[:](mailto:tender@asco.az) tender@asco.az |
|  | **Date and time assigned for the opening of bidding offer envelopes:**  Opening of the envelopes shall take place at **15.00** Baku time on **May 4, 2023** in the address stated in section V of the announcement.  Persons wishing to participate in the opening of the envelopes shall submit a document confirming their permission to participate (the relevant power of attorney from the participating legal entity or natural person) and the ID card at least half an hour before the commencement of the bidding. |
|  | **Information on the winner of the bidding :**  Information on the winner of the bidding will be posted in the "Announcements" section of the ASCO official website. |
|  |  |

**(On the participant`s letter head)**

**APPLICATION FOR PARTICIPATION IN**

**THE OPEN BIDDING**

\_\_\_\_\_\_\_\_\_\_\_ city “\_\_”\_\_\_\_\_\_\_20\_

\_\_\_\_\_\_\_\_\_\_\_№

To the attention of the Chairman of ASCO Procurement Committee

Mr Jabrail Mahmudlu

We, hereby confirm the intention of [ to state full name of the participant ] to participate in the open bidding No. [ bidding No. shall be inserted by participant ] announced by ASCO in respect of procurement of "\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_" .

Moreover, we confirm that no winding - up or bankruptcy proceeding is being performed or there is no circumstance of cessation of activities or any other circumstance that may impede participation of [ to state full name of the participant ] in the stated bidding.

In addition, we warrant that [ to state full name of the participant ] is not an affiliate of ASCO.

Below-mentioned contact details are available to respond to any question that may emerge in relation to the documents submitted and other issues:

* Contact person in charge:
* Position of the contact person:
* Telephone No.:
* E-mail:

**Attachment:**

1. *Original of the bank evidence as a proof of payment of participation fee – \_\_ page(s).*

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

*(initials of the authorized person) (signature of the authorized person)*

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

*(position of the authorized person)*

**STAMP HERE**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| *Item No.* | *Malın adı* | *TECHNICAL SPECIFICATIONS OF MATERIALS* | *MEASUREMENT UNIT* | *Quantity* | *Requisition* | *Vessel / Area name* | *Certification requirement* |
| 1 | Bilge water hose, internal Ø 75 mm, external Ø 89 mm, 16 bar. L - 40 m, complete with camlock coupling at both ends. Ø 75 mm, 20 bar |  | 1 | pcs | 10058439 | R. Hajiyev | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 2 | Iron collar clamp 41 x 47 (with bolt and screw nut) |  | 10 | pcs | 10061368 | S406 | Certificate of conformity and quality |
| 3 | . Iron collar clamp 45 x 49 (with bolt and screw nut) |  | 10 | pcs | 10061368 | S406 | Certificate of conformity and quality |
| 4 | Iron collar clamp 53 x 59 (with bolt and screw nut) |  | 10 | pcs | 10061368 | S406 | Certificate of conformity and quality |
| 5 |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  | Water hose Ø - 32 mm, 50 m, 8 bar ГОСТ 18698 - 79 |  | 1 | pcs | 10062476 | Hovsan | Certificate of conformity and quality |
| 10 | Water hose Ø - 32 mm, 50 m, 8 bar ГОСТ 18698 - 79 |  | 1 | p c s | 10061565 | Zyra | Certificate of conformity and quality |
| 11 | Water hose 75 mm, 16 bar (1 Weco 4 ``coupling) |  | 25 | metre | 10061845 | "Khazar - 3" | Certificate of conformity and quality |
| 12 | Air hose Ø 16 mm equipped with plastic internal side 10 bar |  | 300 | metre | 10061919 | MTF vessels | Certificate of conformity and quality |
| 13 | Durite hose internal dia. Ø 76 mm 10 bar |  | 10 | metre | 10063097 | Bibiheybat Ship Repair Yard - I. Huseynov | Certificate of conformity and quality |
| 14 | Fecal hose 65 mm 12 bar |  | 20 | metre | 10062533 | The Caspian Sea Oil Fleet - KP. Agasiyev | Certificate of conformity and quality |
| 15 |  |  | 40 | metre | 10062869 | The Caspian Se Oil Fleet - "Neftegaz - 64" | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 16 | Sandblaster hose (high pressure resistant) Maximum wear resistance is 60 mm3 according to DIN 53 516:1987. Working pressure is 12 bar. The pressure required to break the hose is 36 bar. Operating temperature range - from -300 to +800 °C. | 32x8mm,12-36bar устойчивый к высокому давлению Максимальная абразивная износостойкость – 60 мм3, что соответствует DIN 53 516:1987. Рабочее давление составляет 12 бар. Давление, необходимое для разрыва рукава, – 36 бар. Диапазон рабочих температур – от -300 до +800 °С. | 500 | metre | 10062080 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 17 | Sandblaster hose ( SUNFLEX AH300 3/4", WP20 BAR / BP 60 bar) high pressure resistant Category: Water hose Showcase: All Showcase Description of Air Hose (AH 300) size 3/4 inch x 1 meter can be for water, wind, gas Features: -. Temperature: -10 ° C to +85 ° C -. Pipe Black, Smooth, TPR material, oil mist resistant -. 1 roll: 100 meters -. Size: working pressure: 300 psi / 20 bar Bruising pressure: 900 psi / 60 bar   ISO: 9001: 2008 | SUNFLEX AH300 3/4",WP20 BAR/BP 60bar устойчивый к высокому давлению Категория: Водяной шланг Витрина: Вся витрина Описание шланга для воздушного шланга (AH 300), размер 3/4 дюйма x 1 метр может быть для воды, ветра, газа Технические характеристики: Температура: от -10 градусов С до +85 градусов С Трубка: черная, гладкая, материал TPR, устойчив к масляному туману 1 рулон: 100 метров -Размер : рабочее давление: 300psi/20 бар  Давление притирания: 900 фунтов/кв. дюйм/60 бар ISO: 9001: 2008 | 400 | metre | 10062080 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 18 | High Pressure Hose Length: 50 ft. (15.2 m) Hose Diameter: 1 / 4 inch. (6.4 mm)  Female NPSM: 1/4 inch. Weight 6.69 lbs Dimensions 15.6 × 17.85 × 3.3 in. Brand: Graco | 500 bar, 1/4", 15,2m (Graco H72550) | 27 | p c s | 10062080 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 19 | High pressure hose Length: 1.4 m - Diameter: 3/16 - Connections : Union Nut 1/4" NPSM Female, 1/4" NPSM Male - Max. allowable working pressure: 227 bar Graco Part Number: 238959 | Graco Bluemax II 227bar,3/16",1,4m Длина: 1,4 м - Диаметр: 3/16 - Соединения: Накидная гайка 1/4" NPSM с внутренней резьбой, 1/4" NPSM с наружной резьбой - Макс. допустимое рабочее давление: 227 бар Артикул Graco: 238959 | 10 | p c s | 10062080 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 20 | Propane hose Ø 8 mm (red color) external diameter Ø 13 mm, 20 bar |  | 300 | metre | 10063530 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 21 | Oxygen hose Ø 8 mm (blue color), external diameter Ø 13 mm, 20 bar |  | 300 | metre | 10063530 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 22 | Fuel hose 16 bar, external Ø 90 mm, internal Ø 70 mm. Equipped with universal coupling at one end. Ø-100 mm: Ø -100 mm hammer coupling at another end |  | 25 | metre | 10063319 | The Caspian Sea Oil Fleet "Khazar-1" | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 23 | Oil hose ø 50 mm |  | 50 | metre | 10063319 | The Caspian Sea Oil Fleet "Khazar-1" | Certificate of conformity and quality |
| 24 | Water hose (wire armored) 32 mm 8 bar |  | 30 | metre | 10063319 | The Caspian Sea Oil Fleet "Khazar-1" | Certificate of conformity and quality |
| 25 | Domestic water hose, external Ø 65 mm, internal Ø 50 mm, 10 bar. Equipped with universal coupling at both ends Coupling: external Ø 162 mm, internal Ø 37 mm. |  | 30 | metre | 10063142 | The Caspian Sea Oil Fleet - PSK 40 | Quality and Conformity Certificate / Certificate issued by the International Maritime Classification Society |
| 26 | Torque Wrench Hose with coupling L = 4 m HTWH4 |  | 4 | p c s | 10062994 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 27 | Water hose (rubber) Ø 15 mm 6 bar |  | 50 | metre | 10062769 | Bibiheybat Ship Repair Yard | Certificate of conformity and quality |
| 28 | Liquefied gas hose H0620 Ø 6 mm (Yildiz) |  | 500 | metre | 10062274 | Bibiheybat Ship Repair Yard | Certificate of conformity and quality |
| 29 | Oxygen hose H0601 Ø 6 mm (Yildir) |  | 500 | metre | 10062274 | Bibiheybat Ship Repair Yard | Certificate of conformity and quality |
| 30 | Air hose Ø 16 mm equipped with plastic internal side 10 bar |  | 600 | metre | 10061086 | Bibiheybat Ship Repair Yard | Certificate of conformity and quality |
| 31 | Durite hose ø 27 mm Structure 40U - 27 - 7 TU 0056016 - 87 "40" - structural group "U" - sleeve type according to the purpose "27" - size of the internal diameter "7" - working pressure of the hose in bar Internal / external diameter: 27 / 36 mm Wall thickness: 4.5 mm Sleeve length: up to 10 m (depending on the batch) Working pressure: up to 7 bar Working temperature: From -55 °С to +100 °С Min. bending radius: 33 cm Base: rubber (internal and external layer) | Дюритовый рукав 27 мм прокладочной конструкции 40У-27-7 ТУ 0056016-87 «40» - конструктивная группа «У» - тип рукава по назначению «27» - размер внутреннего диаметра «7» - рабочее давление рукава в атм Диаметр внутренний / наружный: 27 / 36 мм Толщина стенки:4,5 мм Длина рукава:до 10 м (зависит от партии) Рабочее давление: до 7 бар Рабочая температура: от -55 °С до +100 °С Мин. радиус изгиба:33 см Основа: резина (наружный и внутренний слой) | 30 | metre | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 32 | Durite hose ø 42 mm Structure 40U - 42 - 10 TU 0056016 - 87 "40" - structural group "U" - sleeve type according to the purpose "42" - size of the internal diameter "10" - working pressure of the hose in bar Internal / external diameter: 42 mm Wall thickness: 4.5 mm Sleeve length: up to 10 m (depending on the batch) Working pressure: up to 10 bar Working temperature: From -55 °С to +100 °С Min. bending radius: 33 cm Base: rubber (internal and external layer) | iç diametr ø42 mm Дюритовый рукав 42 мм прокладочной конструкции 40У-42-10 ТУ 0056016-87 «40» - конструктивная группа «У» - тип рукава по назначению «42» - размер внутреннего диаметра «10» - рабочее давление рукава в атм Диаметр внутренний : 42 мм Толщина стенки:4,5 мм Длина рукава:до 10 м (зависит от партии) Рабочее давление: до 10 бар Рабочая температура: от -55 °С до +100 °С Мин. радиус изгиба:33 см Основа: резина (наружный и внутренний слой) | 30 | metre | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 33 | Durite hose ø 50 mm Structure 40U - 50 - 10 TU 0056016 - 87 "40" - structural group "U" - sleeve type according to the purpose "50" - size of the internal diameter "10" - working pressure of the hose in bar Internal / external diameter: 50 mm Wall thickness: 4.5 mm Sleeve length: up to 10 m (depending on the batch) Working pressure: up to 10 bar Working temperature: From -55 °С to +100 °С Min. bending radius: 33 cm Base: rubber (internal and external layer) | Дюритовый рукав 50 мм прокладочной конструкции 40У-50-10 ТУ 0056016-87 «40» - конструктивная группа «У» - тип рукава по назначению «50» - размер внутреннего диаметра «10» - рабочее давление рукава в атм Диаметр внутренний : 50 мм Толщина стенки:4,5 мм Длина рукава:до 10 м (зависит от партии) Рабочее давление: до 10 бар Рабочая температура: от -55 °С до +100 °С Мин. радиус изгиба:33 см Основа: резина (наружный и внутренний слой) | 30 | metre | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 34 | Durite hose ø 48 mm Structure 40U - 48 - 10 TU 0056016 - 87 "40" - structural group "U" - sleeve type according to the purpose "48" - size of the internal diameter "10" - working pressure of the hose in bar Internal diameter: 48 mm Wall thickness: 4.5 mm Sleeve length: up to 10 m (depending on the batch) Working pressure: up to 10 bar Working temperature: From -55 °С to +100 °С Min. bending radius: 33 cm Base: rubber (internal and external layer) | Дюритовый рукав 48 мм прокладочной конструкции 40У-48-10 ТУ 0056016-87 «40» - конструктивная группа «У» - тип рукава по назначению «48» - размер внутреннего диаметра «10» - рабочее давление рукава в атм Диаметр внутренний : 48 мм Толщина стенки:4,5 мм Длина рукава:до 10 м (зависит от партии) Рабочее давление: до 10 бар Рабочая температура: от -55 °С до +100 °С Мин. радиус изгиба:33 см Основа: резина (наружный и внутренний слой) | 30 | metre | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 35 | Durite hose ø 58 mm Structure 40U - 58 - 7 TU 0056016 - 87 "40" - structural group "U" - sleeve type according to the purpose "58" - size of the internal diameter "7" - working pressure of the hose in bar Internal / external diameter: 58 mm Wall thickness: 4.5 mm Sleeve length: up to 10 m (depending on the batch) Working pressure: up to 7 bar Working temperature: From -55 °С to +100 °С Min. bending radius: 33 cm Base: rubber (internal and external layer) | Дюритовый рукав 58 мм прокладочной конструкции 40У-58-7 ТУ 0056016-87 «40» - конструктивная группа «У» - тип рукава по назначению «58» - размер внутреннего диаметра «7» - рабочее давление рукава в атм Диаметр внутренний : 58 мм Толщина стенки:4,5 мм Длина рукава:до 10 м (зависит от партии) Рабочее давление: до 7 бар Рабочая температура: от -55 °С до +100 °С Мин. радиус изгиба:33 см Основа: резина (наружный и внутренний слой) | 30 | metre | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 36 | Durite hose ø 60 mm Structure 40U - 60 - 7 TU 0056016 - 87 "40" - structural group "U" - sleeve type according to the purpose "60" - size of the internal diameter "7" - working pressure of the hose in bar Internal / external diameter: 60 mm Wall thickness: 4.5 mm Sleeve length: up to 10 m (depending on the batch) Working pressure: up to 7 bar Working temperature: From -55 °С to +100 °С Min. bending radius: 33 cm Base: rubber (internal and external layer) | Дюритовый рукав 60 мм прокладочной конструкции 40У-60-7 ТУ 0056016-87 «40» - конструктивная группа «У» - тип рукава по назначению «60» - размер внутреннего диаметра «7» - рабочее давление рукава в атм Диаметр внутренний : 60 мм Толщина стенки:4,5 мм Длина рукава:до 10 м (зависит от партии) Рабочее давление: до 7 бар Рабочая температура: от -55 °С до +100 °С Мин. радиус изгиба:33 см Основа: резина (наружный и внутренний слой) | 25 | metre | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 37 | Durite hose ø 76 mm Structure 40U - 76 - 10 TU 0056016 - 87 "40" - structural group "U" - sleeve type according to the purpose "76" - size of the internal diameter "10" - working pressure of the hose in bar Internal / external diameter: 76 mm Wall thickness: 4.5 mm Sleeve length: up to 10 m (depending on the batch) Working pressure: up to 10 bar Working temperature: From -55 °С to +100 °С Min. bending radius: 33 cm Base: rubber (internal and external layer) | Дюритовый рукав 76 мм прокладочной конструкции 40У-76-10 ТУ 0056016-87 «40» - конструктивная группа «У» - тип рукава по назначению «76» - размер внутреннего диаметра «10» - рабочее давление рукава в атм Диаметр внутренний : 76 мм Толщина стенки:4,5 мм Длина рукава:до 10 м (зависит от партии) Рабочее давление: до 10 бар Рабочая температура: от -55 °С до +100 °С Мин. радиус изгиба:33 см Основа: резина (наружный и внутренний слой) | 20 | metre | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 38 | Durite hose ø 90 mm Structure 40U - 90 - 3 TU 0056016 - 87 "40" - structural group "U" - sleeve type according to the purpose "90" - size of the internal diameter "3" - working pressure of the hose in bar Internal / external diameter: 90 mm Wall thickness: 4.5 mm Sleeve length: up to 10 m (depending on the batch) Working pressure: up to 3 bar Working temperature: From -55 °С to +100 °С Min. bending radius: 33 cm Base: rubber (internal and external layer) | Дюритовый рукав 90 мм прокладочной конструкции 40У-90-3 ТУ 0056016-87 «40» - конструктивная группа «У» - тип рукава по назначению «90» - размер внутреннего диаметра «3» - рабочее давление рукава в атм Диаметр внутренний : 90 мм Толщина стенки:4,5 мм Длина рукава:до 10 м (зависит от партии) Рабочее давление: до 3 бар Рабочая температура: от -55 °С до +100 °С Мин. радиус изгиба:33 см Основа: резина (наружный и внутренний слой) | 20 | metre | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 39 | Iron collar clamp 15-22mm bolt with screw nut (Reinforced single bolt clamp, galvanized steel) | Хомут усиленный одноболтовый, оцинкованная сталь | 100 | p c s | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 40 | Iron collar clamp 20 - 32 mm bolt with screw nut (Reinforced single bolt clamp, galvanized steel) | Хомут усиленный одноболтовый, оцинкованная сталь | 50 | p c s | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 41 | Iron collar clamp 25 - 40 mm bolt with screw nut (Reinforced single bolt clamp, galvanized steel) | |  | | --- | | Хомут усиленный одноболтовый, оцинкованная сталь | | 50 | p c s | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 42 | Iron collar clamp 32 - 50 mm bolt with screw nut (Reinforced single bolt clamp, galvanized steel) | Хомут усиленный одноболтовый, оцинкованная сталь | 50 | p c s | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 43 | Iron collar clamp 40 - 56 mm bolt with screw nut (Reinforced single bolt clamp, galvanized steel) | Хомут усиленный одноболтовый, оцинкованная сталь | 50 | p c s | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 44 | Iron collar clamp 40 - 60 mm bolt with screw nut (Reinforced single bolt clamp, galvanized steel) | Хомут усиленный одноболтовый, оцинкованная сталь | 50 | p c s | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 45 | Iron collar clamp 50 - 70 mm bolt with screw nut (Reinforced single bolt clamp, galvanized steel) | Хомут усиленный одноболтовый, оцинкованная сталь | 50 | p c s | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 46 | Iron collar clamp 60 - 80 mm bolt with screw nut (Reinforced single bolt clamp, galvanized steel) | Хомут усиленный одноболтовый, оцинкованная сталь | 50 | p c s | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 47 | Iron collar clamp 70 - 90 mm bolt with screw nut (Reinforced single bolt clamp, galvanized steel) | Хомут усиленный одноболтовый, оцинкованная сталь | 50 | p c s | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 48 | Iron collar clamp 86 - 91 mm bolt with screw nut (Reinforced single bolt clamp, galvanized steel) | Хомут усиленный одноболтовый, оцинкованная сталь | 30 | p c s | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 49 | Iron collar clamp 87 - 112 mm bolt with screw nut (Reinforced single bolt clamp, galvanized steel) | Хомут усиленный одноболтовый, оцинкованная сталь | 30 | p c s | 10063933 | Zykh Ship Repair and Construction Yard | Certificate of conformity and quality |
| 50 | Water hose (black) 20 х 30 - 1 ГОСТ 10362-2017 |  | 200 | metre | 10062769 | Bibiheybat Ship Repair Yard | Certificate of conformity and quality |
| **51** | Water hose (rubber) Ø 15 mm 6 bar |  | **50** | metre | **10062769** | **Bibiheybat Ship Repair Yard** | **Certificate of conformity and quality** |

|  |  |  |
| --- | --- | --- |
| № | Criteria | Score |
| 1 | Value of the bidding offer :  :   * other Bidding Offers shall be evaluated in accordance with * the following formula for those who have offered the lowest price at the same time:   PFA = MOP / BQT x 80  PFA - points for assessment  MOP - minimum offer price BQT - bidder's quotation | 80  80 |
| 3 | Delivery period:  Within 20 days upon the initial order  More than 20 days | 20  0 |

**Note: Payment condition will be accepted on actual basis only and other conditions rejected.**

**For technical questions please contact :**

**Rza Panaliyev**

**Tel: +99450 6740550**

**E-mail:** [**Rasim.huseynov@asco.az**](mailto:Rasim.huseynov@asco.az)

Due diligence shall be performed in accordance with the Procurement Guidelines of ASCO prior to the conclusion of the purchase agreement with the winner of the bidding.

The company shall enter through this link http: //asco.az/sirket/satinalmalar/podratcilarin-elektron-muraciet-formasi// to complete the special form or submit the following documents:

* Articles of Association of the company (all amendments and changes including)
* An extract from state registry of commercial legal entities (such extract to be issued not later than last 1 month)
* Information on the founder in case if the founder of the company is a legal entity
* Certificate of Tax Payer`s Identification Number
* Audited accounting balance sheet or tax declaration (depending on the taxation system) / reference issued by taxation bodies on non-existence of debts for tax
* Identification card of the legal representative
* Licenses necessary for provision of the relevant services / works (if any)

No agreement of purchase shall be concluded with the company which did not present the above-mentioned documents or failed to be assessed positively as a result of the due diligence performed and shall be excluded from the bidding!